========== Efuse Common Setting ==========
emmc_boot_dis = off
nand_boot_dis = off
nand_boot_speedup_dis = off
pid_vid_custom_en = off
ufs_boot_dis = off
efuse_sf_boot_dis = off
sdmmc_boot_dis = off
sbc_pub_hash_dis = off
sbc_pub_hash1_dis = off
sbc_pub_hash2_dis = off
sbc_pub_hash3_dis = off
sbc_pubk_hash_fa_dis = off
sbc_pubk_hash1_fa_dis = off
sbc_pubk_hash2_fa_dis = off
sbc_pubk_hash3_fa_dis = off
sbc_pubk_hash_mtk_fa_dis = off
fa_mode_en = off
spare = 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 
usbdl_type = 0

========== Efuse Secure Setting ==========
acc_en = off
sbc_en = on
daa_en = off
sla_en = off
ack_en = off
jtag_dis = off
jtag_sw_con = off
rom_cmd_dis = off
dbgport_lock_dis = off
jtag_sec_passwd_en = off
md1_sbc_en = off
c2k_sbc_en = off
pl_ar_en = off
pk_cus_en = off
ac_key = 44332211 88776655 CCBBAA99 FFFFEEDD 
sbc_pub_key_hash = 465B66BB 790C4DAA 62409CD7 7366D4CC 415103D9 86CFDCC6 EE0B0CAC 4DF0E3EA 

========== Efuse Lock Setting ==========
common_ctrl_lock = off
usb_id_lock = off
spare_lock = off
sec_ctrl_lock = off
ackey_lock = off
sbc_pubk_hash_lock = off
sec_msc_lock = off
custk_lock = off
oem_lock = off
sbc_pubk_hash1_lock = off
sbc_pubk_hash2_lock = off
sbc_pubk_hash3_lock = off
cust_crypt_data_lock = off

==========Efuse Extra Setting =======
C_LOCK = 0
C_CTRL_0 = 3003
C_CTRL_1 = 15291
C_DATA_0 = 00000000 00000000 
C_DATA_1 = 00000000 00000000 
C_DATA_2 = 00000000 00000000 
C_DATA_3 = 00000000 00000000 
C_DATA_4 = 00000000 00000000 
C_DATA_5 = 00000000 00000000 
CUSTK = 00000000 00000000 00000000 00000000 

